Table 1. U–Pb SHRIMP analyses of Dom Feliciano Belt detrital zircons

Labels	Site	U	Th	Th/U	204Pb/206Pb	f206	238U/206Pb	207Pb/206Pb	206Pb/238U	207Pb/206Pb	conc.*	
		ppm	ppm						corr.			corr.			age			age			%	
Ribeira Belt - Itaiacoca Gp (32928)																			
1.1	m,hd,ov	321	173	0.54	0.00001	±	0.00001	0.0002	1.411	±	0.043	0.3065	±	0.0007	3453	±	82	3503	±	3	99	
2.1	m,osc,ov	70	35	0.49	0.00002	±	0.00009	0.0003	1.514	±	0.045	0.2532	±	0.0029	3269	±	77	3205	±	18	102	
3.1	m,osc,ov	118	92	0.78	0.00009	±	0.00004	0.0016	2.409	±	0.073	0.1360	±	0.0014	2238	±	58	2177	±	17	103	
3.2	m,osc,ov	45	61	1.36	0.00024	±	0.00011	0.0042	2.596	±	0.092	0.1368	±	0.0025	2100	±	64	2187	±	32	96	
4.1	m,osc,ov	41	47	1.17	0.00038	±	0.00012	0.0067	2.472	±	0.088	0.1353	±	0.0021	2190	±	67	2168	±	28	101	
5.1	m,osc,rp	49	45	0.93	0.00006	±	0.00005	0.0011	2.384	±	0.076	0.1368	±	0.0011	2258	±	61	2187	±	14	103	
6.1	m,osc,ov,fr	47	31	0.66	0.00002	±	0.00007	0.0004	2.413	±	0.072	0.1360	±	0.0015	2235	±	57	2177	±	20	103	
7.1	e,osc,ov	97	127	1.31	0.00058	±	0.00008	0.0104	2.897	±	0.102	0.1230	±	0.0019	1912	±	59	2000	±	28	96	
8.1	e,osc,p,fr	101	66	0.65	0.00001	±	0.00003	0.0002	2.379	±	0.078	0.1417	±	0.0008	2262	±	63	2248	±	10	101	
9.1	m,osc,ov	40	31	0.79	0.00000	±	0.00002	0.0001	2.376	±	0.085	0.1414	±	0.0023	2265	±	69	2244	±	29	101	
12.1	m,hd,ov	412	320	0.78	0.00033	±	0.00003	0.0059	3.476	±	0.096	0.1256	±	0.0007	1630	±	40	2037	±	11	80	
13.1	e,hd,ov	447	349	0.78	0.00035	±	0.00003	0.0063	4.022	±	0.111	0.1165	±	0.0010	1431	±	36	1903	±	15	75	
14.1	m,osc,ov	47	36	0.75	0.00001	±	0.00006	0.0002	2.523	±	0.078	0.1370	±	0.0016	2152	±	57	2189	±	21	98	
15.1	e,osc,p	796	497	0.63	0.00081	±	0.00020	0.0145	3.177	±	0.137	0.1275	±	0.0040	1764	±	67	2063	±	56	86	
16.1	m,osc,ov,fr	31	32	1.05	0.00001	±	0.00005	0.0002	2.427	±	0.083	0.1373	±	0.0022	2224	±	65	2194	±	28	101	
17.1	m,osc,p,fr	33	22	0.66	0.00001	±	0.00004	0.0002	2.570	±	0.085	0.1265	±	0.0012	2119	±	60	2050	±	17	103	
18.1	m,osc,rp	76	51	0.67	0.00043	±	0.00008	0.0077	2.897	±	0.091	0.1215	±	0.0017	1912	±	52	1979	±	25	97	
Ribeira Belt – Antinha Fm (34537)																				
1.1	e,h,osc,rp	28	42	1.47	0.00034	±	0.00042	0.0060	3.210	±	0.213	0.1093	±	0.0072	1748	±	102	1787	±	124	98	
2.1	e,osc,rp	595	1318	2.21	0.00293	±	0.00035	0.0521	7.299	±	0.380	0.1131	±	0.0064	828	±	41	1850	±	106	45	
3.1	m/c,osc,p	81	42	0.51	0.00054	±	0.00015	0.0097	2.483	±	0.102	0.1365	±	0.0041	2182	±	76	2183	±	53	100	
3.2	e,osc,p	70	38	0.55	0.00009	±	0.00014	0.0016	2.486	±	0.109	0.1406	±	0.0029	2180	±	81	2234	±	36	98	
4.1	e,osc,p	341	346	1.01	0.00043	±	0.00013	0.0076	10.225	±	0.294	0.0534	±	0.0026	601	±	17	346	±	113	174	
5.1	e,h,osc,rp	199	111	0.56	0.00000	±	0.00000	0.0000	2.697	±	0.079	0.1329	±	0.0011	2033	±	52	2136	±	15	95	
6.1	e,h,rp	97	132	1.37	0.00085	±	0.00023	0.0152	3.074	±	0.096	0.1229	±	0.0040	1816	±	50	1999	±	59	91	
7.1	m/c,h,p	341	230	0.68	0.00534	±	0.00091	0.0951	5.268	±	0.369	0.0489	±	0.0152	1120	±	72	143	±	958	782	
8.1	e,osc,h,rp	138	337	2.43	0.00001	±	0.00002	0.0002	2.804	±	0.104	0.1252	±	0.0022	1966	±	63	2032	±	31	97	
9.1	e,osc,p	141	77	0.55	0.00055	±	0.00055	0.0098	10.311	±	0.530	0.0577	±	0.0094	597	±	29	518	±	404	115	
10.1	e,osc,fr	108	51	0.47	0.00009	±	0.00009	0.0015	2.625	±	0.084	0.1351	±	0.0021	2081	±	57	2165	±	27	96	
11.1	e,osc,p	272	271	1.00	0.00045	±	0.00025	0.0079	10.363	±	0.423	0.0579	±	0.0048	594	±	23	524	±	192	113	
12.1	e,osc,rp	622	191	0.31	0.00093	±	0.00013	0.0165	3.783	±	1.237	0.1183	±	0.0050	1512	±	457	1931	±	78	78	
13.1	m,osc,p,fr	920	258	0.28	0.00081	±	0.00026	0.0144	8.761	±	0.257	0.0566	±	0.0046	697	±	19	474	±	189	147	
7.2	m/c,h,p	356	203	0.57	0.00391	±	0.00061	0.0695	4.821	±	0.729	0.0625	±	0.0120	1215	±	170	690	±	474	176	
14.1	e,osc,p	275	142	0.51	0.00029	±	0.00010	0.0052	2.452	±	0.158	0.1364	±	0.0055	2205	±	121	2183	±	72	101	
15.1	e,osc,p	158	102	0.65	0.00081	±	0.00064	0.0145	10.431	±	0.375	0.0599	±	0.0105	590	±	20	599	±	433	98	
16.1	m,osc,ov	146	86	0.59	0.00023	±	0.00010	0.0042	2.147	±	0.109	0.1567	±	0.0024	2465	±	105	2420	±	26	102	
Ribeira Belt - Votuverava Fm (34536)																			
1.1	e,osc,h,rp	35	20	0.56	0.00001	±	0.00002	0.0002	2.035	±	0.082	0.1605	±	0.0036	2577	±	86	2461	±	39	105	
2.1	m,osc,ov	90	76	0.84	0.00014	±	0.00014	0.0021	2.398	±	0.071	0.1383	±	0.0038	2247	±	56	2206	±	49	102	
3.1	m,osc,ov	76	67	0.89	0.00014	±	0.00023	0.0021	2.645	±	0.090	0.1282	±	0.0043	2067	±	61	2074	±	61	100	
4.1	m,h,ov	90	111	1.24	0.00001	±	0.00001	0.0002	2.245	±	0.077	0.1438	±	0.0041	2375	±	69	2273	±	50	105	
5.1	m,osc,ov	46	33	0.72	0.00007	±	0.00016	0.0011	2.666	±	0.094	0.1260	±	0.0044	2053	±	62	2043	±	63	101	
6.1	m,osc,ov	170	108	0.63	0.00007	±	0.00008	0.0011	2.436	±	0.094	0.1373	±	0.0016	2218	±	72	2193	±	20	101	
7.1	m,osc,h,fr	305	115	0.38	0.00026	±	0.00005	0.0039	2.731	±	0.064	0.1329	±	0.0011	2011	±	41	2136	±	14	94	
8.1	m,osc,o	551	179	0.32	0.00061	±	0.00011	0.0092	3.123	±	0.106	0.1238	±	0.0055	1791	±	53	2011	±	81	89	
9.1	m,osc,h,rp	146	127	0.87	0.00005	±	0.00008	0.0008	2.106	±	0.069	0.1620	±	0.0017	2505	±	68	2476	±	18	101	
10.1	e,osc,h,ov	233	92	0.39	0.00009	±	0.00003	0.0013	2.595	±	0.084	0.1282	±	0.0012	2101	±	59	2073	±	17	101	
11.1	m,osc,h,ov	16	16	0.95	0.00001	±	0.00004	0.0002	3.097	±	0.695	0.1382	±	0.0072	1804	±	363	2205	±	93	82	
12.1	m,h,fr	64	28	0.44	0.00002	±	0.00006	0.0004	1.464	±	0.043	0.2582	±	0.0027	3356	±	77	3236	±	16	104	
13.1	m,osc,rp,fr	41	43	1.07	0.00001	±	0.00002	0.0002	3.150	±	0.139	0.1070	±	0.0054	1777	±	69	1749	±	96	102	
14.1	e,osc,ov	111	52	0.47	0.00001	±	0.00002	0.0002	2.354	±	0.075	0.1342	±	0.0017	2282	±	62	2154	±	22	106	
15.1	m,osc,rp	104	72	0.70	0.00006	±	0.00017	0.0008	3.358	±	0.134	0.1078	±	0.0034	1680	±	59	1762	±	59	95	
16.1	m,osc,rp	177	155	0.88	0.00001	±	0.00003	0.0002	2.373	±	0.073	0.1370	±	0.0011	2267	±	59	2189	±	14	104	
17.1	e,osc,h,rp	591	470	0.80	0.00074	±	0.00006	0.0112	3.837	±	0.084	0.1266	±	0.0012	1493	±	29	2051	±	17	73	
18.1	m,osc,ov	125	112	0.89	0.00030	±	0.00009	0.0045	2.523	±	0.094	0.1351	±	0.0031	2152	±	68	2165	±	40	99	
19.1	m,osc,fr	170	79	0.47	0.00053	±	0.00012	0.0081	2.361	±	0.066	0.1344	±	0.0024	2277	±	54	2156	±	32	106	
20.1	m,osc,ov	227	112	0.49	0.00001	±	0.00004	0.0002	1.837	±	0.055	0.1956	±	0.0011	2802	±	68	2790	±	9	100	
21.1	m,osc,h,ov	241	124	0.52	0.00015	±	0.00005	0.0023	2.436	±	0.062	0.1379	±	0.0020	2217	±	48	2201	±	25	101	
22.1	m,osc,h,rp	587	229	0.39	0.00024	±	0.00006	0.0036	2.820	±	0.103	0.1272	±	0.0015	1957	±	62	2060	±	21	95	
Ribeira Belt - Capiru Fm (32967)																				
1.1	e,osc,p	67	39	0.58	0.00033	±	0.00008	0.0050	2.426	±	0.111	0.1359	±	0.0020	2225	±	87	2176	±	26	102	
2.1	e,osc,rp	110	55	0.50	0.00012	±	0.00013	0.0018	2.423	±	0.065	0.1355	±	0.0024	2228	±	51	2170	±	31	103	
3.1	m,osc,p,fr	83	45	0.54	0.00014	±	0.00006	0.0022	2.429	±	0.087	0.1379	±	0.0014	2222	±	68	2201	±	18	101	
4.1	m,osc,ov	43	28	0.66	0.00014	±	0.00012	0.0021	2.476	±	0.082	0.1363	±	0.0025	2187	±	61	2181	±	32	100	
5.1	e,osc,fr,rp	180	116	0.65	0.00167	±	0.00012	0.0252	2.849	±	0.078	0.1243	±	0.0034	1939	±	46	2019	±	50	96	
6.1	e,osc,ov	86	59	0.69	0.00023	±	0.00020	0.0035	2.483	±	0.098	0.1358	±	0.0037	2182	±	74	2174	±	48	100	
7.1	e,osc,rp	74	50	0.68	0.00041	±	0.00022	0.0062	2.240	±	0.104	0.1364	±	0.0055	2379	±	93	2182	±	71	109	
8.1	e,osc,ov	625	626	1.00	0.01201	±	0.00071	0.1816	9.200	±	0.501	0.0966	±	0.0161	665	±	34	1560	±	349	43	
9.1	e,osc,rp	100	59	0.59	0.00001	±	0.00002	0.0002	2.445	±	0.093	0.1367	±	0.0027	2210	±	71	2185	±	34	101	
10.1	m,h,rp	404	224	0.56	0.00172	±	0.00015	0.0260	3.344	±	0.108	0.1252	±	0.0026	1687	±	48	2031	±	37	83	
11.1	m,h,ov	216	160	0.74	0.00001	±	0.00002	0.0002	1.625	±	0.073	0.2326	±	0.0034	3092	±	111	3070	±	23	101	
12.1	m,osc,ov	231	81	0.35	0.00061	±	0.00013	0.0092	2.994	±	0.144	0.1283	±	0.0023	1858	±	78	2075	±	32	90	
13.1	e,osc,ov	88	52	0.59	0.00041	±	0.00016	0.0062	2.356	±	0.099	0.1338	±	0.0031	2281	±	81	2149	±	40	106	
14.1	e,h,ov	1251	523	0.42	0.00065	±	0.00007	0.0099	4.326	±	0.161	0.1464	±	0.0014	1341	±	45	2305	±	16	58	
15.1	e,osc,p,fr	94	85	0.90	0.00016	±	0.00012	0.0025	2.380	±	0.090	0.1351	±	0.0024	2262	±	72	2165	±	31	105	
16.1	e,osc,rp	359	217	0.60	0.00209	±	0.00017	0.0316	2.956	±	0.115	0.2037	±	0.0034	1879	±	64	2856	±	27	66	
17.1	e,osc,rp	237	165	0.69	0.00090	±	0.00014	0.0136	2.865	±	0.109	0.2081	±	0.0034	1930	±	64	2891	±	27	67	
DFB – Brusque Gp (SC 1)																			
1.1	m,osc,p,fr	38	33	0.86	0.00011	±	0.00013	0.0019	2.365	±	0.077	0.1395	±	0.0024	2274	±	63	2221	±	29	102	
1.2	m,osc,p	58	28	0.48	0.00004	±	0.00021	0.0006	2.178	±	0.092	0.1401	±	0.0045	2435	±	86	2229	±	56	109	
2.1	m,osc,p	1384	398	0.29	0.00092	±	0.00006	0.0163	17.364	±	0.482	0.0588	±	0.0013	361	±	10	558	±	49	65	
3.1	m,osc,p	151	88	0.58	0.00021	±	0.00008	0.0037	4.302	±	0.134	0.0945	±	0.0026	1347	±	38	1518	±	52	89	
4.1	m,osc,fr	11	3	0.24	0.00046	±	0.00042	0.0082	2.593	±	0.107	0.1202	±	0.0074	2103	±	75	1960	±	114	107	
5.1	m,osc,hd,p,fr	1057	532	0.50	0.00039	±	0.00005	0.0069	12.526	±	0.358	0.0631	±	0.0016	495	±	14	713	±	53	70	
6.1	e,osc,p/eq	69	38	0.55	0.00001	±	0.00002	0.0002	2.673	±	0.079	0.1263	±	0.0024	2048	±	52	2047	±	34	100	
7.1	c,hb,eq	204	79	0.39	0.00027	±	0.00007	0.0047	10.708	±	0.474	0.0630	±	0.0025	576	±	24	708	±	85	81	
8.1	e/m,hb,eq	52	25	0.49	0.00146	±	0.00036	0.0260	11.348	±	0.915	0.0662	±	0.0076	544	±	42	812	±	259	67	
DFB – Brusque Gp (32929)																			
1.1	m,osc,hd,p,fr	138	62	0.45	0.00038	±	0.00012	0.0068	5.167	±	0.155	0.0786	±	0.0023	1141	±	32	1163	±	59	98	
2.1	e,osc,p,fr	264	133	0.50	0.00019	±	0.00004	0.0034	3.048	±	0.091	0.1094	±	0.0012	1829	±	48	1790	±	19	102	
3.1	m,osc,p,fr	96	32	0.34	0.00001	±	0.00003	0.0002	3.810	±	0.116	0.0938	±	0.0010	1503	±	41	1504	±	19	100	
4.1	m,hb,ov	15	13	0.87	0.00013	±	0.00024	0.0023	5.658	±	0.212	0.0857	±	0.0061	1049	±	36	1332	±	145	79	
5.1	e,osc,rp	62	89	1.44	0.00203	±	0.00040	0.0361	5.141	±	0.189	0.0805	±	0.0075	1146	±	39	1208	±	195	95	
6.1	e,osc,p	107	93	0.87	0.00006	±	0.00011	0.0011	3.130	±	0.094	0.1153	±	0.0024	1787	±	47	1885	±	38	95	
7.1	e,osc,p,fr	63	51	0.81	0.00001	±	0.00003	0.0002	5.274	±	0.177	0.0803	±	0.0014	1119	±	35	1204	±	35	93	
8.1	m,hb,osc,fr	12	10	0.78	0.00167	±	0.00089	0.0297	4.596	±	0.246	0.0847	±	0.0144	1269	±	62	1308	±	373	97	
9.1	e,osc,hd,p,fr	99	65	0.65	0.00026	±	0.00009	0.0046	3.269	±	0.101	0.1124	±	0.0016	1721	±	47	1839	±	26	94	
10.1	e,osc,hd,p,fr	98	36	0.36	0.00001	±	0.00004	0.0002	3.754	±	0.120	0.0941	±	0.0010	1523	±	43	1511	±	20	101	
11.1	e,osc,p,fr	123	183	1.49	0.00004	±	0.00007	0.0007	4.921	±	0.181	0.0807	±	0.0015	1193	±	40	1213	±	37	98	
12.1	m,osc,p,fr	206	149	0.72	0.00019	±	0.00006	0.0034	3.640	±	0.150	0.1072	±	0.0013	1565	±	57	1753	±	22	89	
13.1	e,osc,hd,p,fr	108	43	0.40	0.00004	±	0.00007	0.0007	3.913	±	0.125	0.0894	±	0.0013	1467	±	42	1412	±	29	104	
DFB – Porongos Gp (BRAF 34)																			
1.1	e,h,r	440	53	0.12	0.00157	±	0.00033	0.0278	4.997	±	0.157	0.1105	±	0.0060	1176	±	34	1808	±	103	65	
1.2	e,h,r	377	127	0.34	0.00008	±	0.00004	0.0013	2.521	±	0.069	0.1337	±	0.0012	2154	±	50	2148	±	16	100	
2.1	e,osc,rp	551	217	0.39	0.00038	±	0.00009	0.0068	4.096	±	0.120	0.1177	±	0.0016	1408	±	37	1922	±	25	73	
3.1	e,sz,abr	85	32	0.37	0.00058	±	0.00039	0.0102	2.638	±	0.102	0.1534	±	0.0067	2072	±	69	2384	±	76	87	
4.1	e,osc,fr	40	44	1.09	0.00065	±	0.00027	0.0116	2.863	±	0.159	0.1251	±	0.0051	1931	±	93	2030	±	74	95	
5.1	e,h,p	2147	263	0.12	0.00019	±	0.00004	0.0034	9.868	±	0.279	0.0603	±	0.0008	622	±	17	613	±	27	102	
6.1	e,osc,rp	163	86	0.53	0.00125	±	0.00030	0.0221	6.013	±	0.194	0.0624	±	0.0051	992	±	30	689	±	184	144	
5.2	e,p	1984	167	0.08	0.00011	±	0.00004	0.0019	9.896	±	0.272	0.0608	±	0.0009	621	±	16	632	±	31	98	
7.1	sz,p,fr	494	223	0.45	0.00052	±	0.00014	0.0092	8.746	±	0.336	0.0651	±	0.0024	698	±	25	777	±	78	90	
8.1	e,sz,p,fr	848	854	1.01	0.00033	±	0.00014	0.0058	4.646	±	0.169	0.1188	±	0.0024	1257	±	42	1939	±	36	65	
7.2	e,sz,p	346	141	0.41	0.00016	±	0.00009	0.0028	7.569	±	0.219	0.0664	±	0.0019	800	±	22	819	±	61	98	
10.1	e,sz	245	199	0.81	0.00015	±	0.00012	0.0026	3.194	±	0.109	0.1110	±	0.0025	1756	±	52	1816	±	42	97	
11.1	e,osc,p	79	92	1.17	0.00036	±	0.00015	0.0065	2.716	±	0.100	0.1244	±	0.0031	2021	±	64	2020	±	45	100	
12.1	m,osc,rp	161	61	0.38	0.00015	±	0.00014	0.0027	4.651	±	0.099	0.0846	±	0.0027	1256	±	24	1307	±	63	96	
13.1	e,osc,rp	362	472	1.31	0.00025	±	0.00009	0.0045	2.444	±	0.110	0.1186	±	0.0038	2211	±	85	1935	±	58	114	
14.1	e,osc,p	416	350	0.84	0.00000	±	0.00001	0.0000	1.957	±	0.036	0.1724	±	0.0011	2661	±	40	2581	±	11	103	
15.1	e,osc,p	221	87	0.40	0.00000	±	0.00005	0.0000	4.797	±	0.121	0.0827	±	0.0026	1221	±	28	1262	±	63	97	
16.1	e,osc,rp	416	259	0.62	0.00030	±	0.00009	0.0054	3.803	±	0.121	0.0939	±	0.0017	1505	±	43	1505	±	34	100	
17.1	m,osc,rp	216	70	0.32	0.00017	±	0.00016	0.0030	4.597	±	0.094	0.0823	±	0.0027	1269	±	24	1252	±	65	101	
18.1	osc,r	239	210	0.88	0.00007	±	0.00006	0.0012	2.832	±	0.061	0.1228	±	0.0020	1949	±	36	1997	±	29	98	
19.1	osc,ov	125	95	0.76	0.00021	±	0.00009	0.0037	3.743	±	0.125	0.0966	±	0.0030	1527	±	45	1560	±	59	98	
20.1	osc,ov	76	35	0.47	0.00012	±	0.00012	0.0021	3.012	±	0.102	0.1145	±	0.0043	1848	±	55	1873	±	70	99	
21.1	e,osc,	218	172	0.79	0.00274	±	0.00061	0.0486	10.362	±	0.295	0.0214	±	0.0101	594	±	16	0	±	0	0	
DFB -Lavalleja - Fuente del Puma  (URPR 68)																	
1.1	e,osc,rp	336	276	0.82	0.00010	±	0.00003	0.0018	2.645	±	0.160	0.1265	±	0.0031	2067	±	108	2050	±	44	101	
2.1	e,sz,p	262	96	0.37	0.00030	±	0.00010	0.0054	8.525	±	0.328	0.0630	±	0.0021	715	±	26	707	±	74	101	
3.1	c,osc,r	89	47	0.53	0.00020	±	0.00008	0.0035	1.968	±	0.077	0.1886	±	0.0036	2649	±	86	2730	±	32	97	
4.1	e,osc,rp	391	195	0.50	0.00012	±	0.00009	0.0022	5.582	±	0.172	0.0721	±	0.0021	1062	±	30	990	±	60	107	
5.1	e,osc,rp,r	184	63	0.34	0.00023	±	0.00020	0.0041	10.242	±	0.365	0.0768	±	0.0038	601	±	20	1116	±	102	54	
6.1	e,ov,r	201	149	0.74	0.00189	±	0.00022	0.0335	1.488	±	0.057	0.2198	±	0.0045	3314	±	100	2979	±	33	111	
7.1	e,osc,p	1111	1430	1.29	0.00543	±	0.00048	0.0963	18.349	±	0.668	0.0608	±	0.0090	342	±	12	633	±	354	54	
8.1	c,ov,osc	247	96	0.39	0.00048	±	0.00016	0.0085	9.929	±	0.297	0.0558	±	0.0029	619	±	18	444	±	119	139	
9.1	c,osc,abr	149	139	0.93	0.00034	±	0.00020	0.0060	2.227	±	0.085	0.1520	±	0.0036	2391	±	77	2368	±	40	101	
10.1	e,osc,ov	132	61	0.46	0.00026	±	0.00008	0.0046	1.807	±	0.069	0.2197	±	0.0036	2839	±	88	2978	±	27	95	
11.1	e,osc,p	156	130	0.83	0.00085	±	0.00014	0.0150	2.750	±	0.091	0.1131	±	0.0027	1999	±	57	1850	±	43	108	
12.1	c,osc,rp	517	394	0.76	0.00234	±	0.00018	0.0415	3.149	±	0.106	0.2247	±	0.0033	1778	±	52	3015	±	24	59	
13.1	e,p	157	51	0.32	0.00088	±	0.00034	0.0157	1.677	±	0.099	0.1908	±	0.0063	3014	±	144	2749	±	55	110	
14.1	e,osc,p	150	60	0.40	0.00029	±	0.00018	0.0051	1.579	±	0.049	0.1971	±	0.0038	3162	±	78	2802	±	32	113	
8.2	e,osc,ov	534	302	0.57	0.00137	±	0.00028	0.0243	9.936	±	0.282	0.0635	±	0.0046	618	±	17	724	±	162	85	
15.1	e,ov	190	175	0.92	0.00015	±	0.00005	0.0026	2.665	±	0.084	0.1243	±	0.0014	2054	±	56	2019	±	20	102	
16.1	e,osc	130	63	0.49	0.00037	±	0.00012	0.0066	1.845	±	0.057	0.1867	±	0.0029	2792	±	70	2713	±	25	103	
17.1	e,p	44	39	0.90	0.00032	±	0.00014	0.0057	3.100	±	0.117	0.1109	±	0.0041	1802	±	60	1814	±	69	99	
18.1	osc,fr,ov	98	98	1.00	0.00327	±	0.00033	0.0579	2.497	±	0.123	0.1565	±	0.0062	2171	±	91	2418	±	68	90	
14.2	e,p,h	46	74	1.60	0.00163	±	0.00042	0.0289	2.704	±	0.112	0.1035	±	0.0077	2029	±	72	1687	±	143	120	
19.1	c,h,p	202	129	0.64	0.00017	±	0.00005	0.0029	1.425	±	0.041	0.3180	±	0.0033	3427	±	76	3560	±	16	96	
20.1	e,h,ov	193	121	0.62	0.00009	±	0.00006	0.0015	2.693	±	0.087	0.1253	±	0.0024	2036	±	57	2033	±	34	100	
21.1	e,rp	224	79	0.35	0.00058	±	0.00016	0.0102	2.008	±	0.062	0.1767	±	0.0035	2606	±	67	2622	±	33	99	
DFB - Lavaleja - Zanja del Tigre (URPR 69)																	
1.1	e,osc,rp	260	130	0.50	0.00013	±	0.00005	0.0023	2.536	±	0.086	0.1386	±	0.0026	2143	±	62	2209	±	33	97	
2.1	e,osc,p	143	111	0.77	0.00010	±	0.00006	0.0019	2.456	±	0.077	0.1437	±	0.0020	2202	±	59	2272	±	24	97	
3.1	osc,r	159	47	0.30	0.00005	±	0.00002	0.0008	1.814	±	0.064	0.2233	±	0.0026	2830	±	81	3005	±	19	94	
4.1	e,osc,rp	257	115	0.45	0.00005	±	0.00003	0.0008	2.633	±	0.085	0.1354	±	0.0020	2075	±	57	2169	±	26	96	
5.1	osc,rp	289	62	0.22	0.00011	±	0.00006	0.0019	1.824	±	0.054	0.2137	±	0.0014	2818	±	68	2933	±	11	96	
6.1	m,osc,rp	431	42	0.10	0.00021	±	0.00007	0.0038	2.707	±	0.078	0.1363	±	0.0019	2026	±	51	2181	±	24	93	
7.1	osc,ov	274	144	0.53	0.00019	±	0.00005	0.0034	2.716	±	0.086	0.2248	±	0.0040	2021	±	55	3016	±	29	67	
8.1	osc,ov,fr	327	207	0.63	0.00005	±	0.00005	0.0010	1.389	±	0.069	0.2755	±	0.0029	3495	±	135	3338	±	17	105	
9.1	osc,ov	760	68	0.09	0.00012	±	0.00002	0.0021	2.456	±	0.065	0.1989	±	0.0013	2202	±	50	2817	±	11	78	
10.1	osc,ov	202	78	0.39	0.00020	±	0.00011	0.0036	1.705	±	0.058	0.2216	±	0.0025	2975	±	81	2993	±	18	99	
11.1	p	479	167	0.35	0.00010	±	0.00003	0.0017	2.311	±	0.076	0.1939	±	0.0011	2318	±	64	2775	±	9	84	
12.1	e,osc,rp	132	50	0.38	0.00016	±	0.00006	0.0029	1.570	±	0.061	0.2596	±	0.0033	3177	±	99	3244	±	20	98	
13.1	e,osc,ov	195	94	0.48	0.00012	±	0.00005	0.0021	1.663	±	0.050	0.2229	±	0.0017	3035	±	73	3002	±	12	101	
14.1	osc,ov	244	87	0.36	0.00012	±	0.00005	0.0021	1.452	±	0.107	0.2140	±	0.0018	3378	±	196	2936	±	13	115	
15.1	osc,p,e	614	300	0.49	0.00045	±	0.00007	0.0080	4.136	±	0.128	0.1951	±	0.0018	1396	±	39	2786	±	16	50	
16.1	c,rp,osc	74	32	0.43	0.00041	±	0.00035	0.0073	1.998	±	0.090	0.1939	±	0.0073	2616	±	98	2775	±	63	94	
17.1	e,osc,ov	33	19	0.59	0.00076	±	0.00072	0.0134	2.644	±	0.134	0.1373	±	0.0125	2068	±	90	2194	±	167	94	
18.1	osc,ov	157	65	0.42	0.00009	±	0.00003	0.0017	1.712	±	0.077	0.2085	±	0.0014	2965	±	108	2894	±	11	103	
19.1	e,osc,p	61	91	1.49	0.00025	±	0.00019	0.0044	3.101	±	0.116	0.1046	±	0.0038	1802	±	59	1707	±	68	106	
20.1	c,ov,r	246	34	0.14	0.00018	±	0.00014	0.0032	2.417	±	0.095	0.1926	±	0.0047	2232	±	74	2764	±	40	81	
Damara Belt - Nosib Gp -	 (NP116)																				
1.1	m,abr,hb,	57	51	0.91	0.00024	±	0.00018	0.0041	6.319	±	0.183	0.0704	±	0.0032	947	±	26	941	±	95	101	
2.1	e,abr,hd	146	78	0.53	0.00054	±	0.00014	0.0093	8.191	±	0.203	0.0784	±	0.0027	743	±	17	1157	±	70	64	
3.1	m,hd,osc,p	53	49	0.93	0.00017	±	0.00011	0.0029	4.883	±	0.126	0.0883	±	0.0028	1201	±	28	1388	±	62	87	
4.1	e,osc,rp	115	85	0.74	0.00018	±	0.00005	0.0031	3.173	±	0.079	0.1128	±	0.0019	1766	±	39	1844	±	31	96	
5.1	e,osc,hb,p	213	60	0.28	0.00006	±	0.00004	0.0010	4.848	±	0.073	0.0808	±	0.0009	1209	±	17	1216	±	23	99	
6.1	m,rp,osc,hd	353	137	0.39	0.00001	±	0.00001	0.0002	4.469	±	0.122	0.0840	±	0.0007	1302	±	32	1292	±	17	101	
7.1	m,osc,hd,p	191	149	0.78	0.00005	±	0.00002	0.0009	2.920	±	0.041	0.1179	±	0.0007	1898	±	23	1925	±	11	99	
8.1	e,osc,p	126	43	0.34	0.00003	±	0.00003	0.0006	4.874	±	0.132	0.0822	±	0.0022	1203	±	30	1251	±	53	96	
9.1	e,abr,h,osc	89	52	0.58	0.00029	±	0.00008	0.0050	4.921	±	0.107	0.0773	±	0.0021	1193	±	24	1130	±	56	106	
10.1	e,hb,osc,p	40	31	0.78	0.00054	±	0.00021	0.0092	5.725	±	0.178	0.0680	±	0.0036	1038	±	30	869	±	115	119	
11.1	e/m,abr,hb,osc	74	34	0.46	0.00017	±	0.00015	0.0028	5.008	±	0.118	0.0848	±	0.0027	1174	±	25	1311	±	62	90	
12.1	e/m,hb,osc,p	104	71	0.69	0.00052	±	0.00010	0.0089	4.802	±	0.095	0.0757	±	0.0020	1219	±	22	1087	±	55	112	
DFB – Quecaba Fm  (BRAF 244)																			
1.1	m,osc,p,fr	234	68	0.29	0.00018	±	0.00005	0.0030	3.332	±	0.168	0.1069	±	0.0017	1692	±	75	1748	±	28	97	
2.1	e,osc,p,fr	169	139	0.82	0.00006	±	0.00005	0.0011	2.820	±	0.128	0.1227	±	0.0018	1956	±	77	1996	±	26	98	
3.1	m,hp,p	243	101	0.42	0.00000	±	0.00004	0.0000	4.197	±	0.139	0.0858	±	0.0014	1378	±	41	1335	±	31	103	
4.1	e,osc,p	133	107	0.81	0.00000	±	0.00009	0.0000	2.927	±	0.116	0.1145	±	0.0020	1895	±	65	1872	±	32	101	
5.1	e,osc,p,fr	434	102	0.23	0.00004	±	0.00002	0.0007	3.767	±	0.112	0.0937	±	0.0011	1518	±	40	1503	±	23	101	
6.1	m,hp,p	316	118	0.37	0.00004	±	0.00005	0.0007	4.389	±	0.112	0.0842	±	0.0016	1323	±	31	1296	±	37	102	
7.1	e,osc,p	681	421	0.62	0.00031	±	0.00006	0.0050	4.818	±	0.144	0.0797	±	0.0012	1216	±	33	1189	±	29	102	
8.1	m,hd,p	393	144	0.37	0.00006	±	0.00003	0.0010	4.740	±	0.121	0.0807	±	0.0011	1234	±	29	1215	±	28	102	
9.1	m,hp,p	304	93	0.31	0.00008	±	0.00007	0.0013	4.988	±	0.152	0.0791	±	0.0015	1178	±	33	1174	±	38	100	
10.1	e,hd,p,fr	693	40	0.06	0.00032	±	0.00009	0.0053	4.298	±	0.465	0.0875	±	0.0022	1348	±	133	1372	±	50	98	
11.1	m,hp,p,fr	367	82	0.22	0.00036	±	0.00012	0.0060	5.802	±	0.197	0.0696	±	0.0021	1025	±	32	916	±	63	112	
12.1	m,osc,p	320	94	0.29	0.00013	±	0.00007	0.0022	5.082	±	0.148	0.0782	±	0.0016	1158	±	31	1153	±	41	100	
13.1	m,hd,p,fr	319	182	0.57	0.00001	±	0.00004	0.0002	2.947	±	0.081	0.1146	±	0.0013	1883	±	45	1873	±	21	101	
14.1	e,osc,p,fr	579	243	0.42	0.00043	±	0.00008	0.0071	3.096	±	0.116	0.1128	±	0.0021	1804	±	59	1845	±	34	98	
15.1	m,hd,p	472	53	0.11	0.00124	±	0.00014	0.0205	3.149	±	0.094	0.1062	±	0.0026	1778	±	46	1736	±	46	102	
16.1	m,h,p,fr	296	189	0.64	0.00100	±	0.00017	0.0165	2.927	±	0.101	0.1139	±	0.0031	1895	±	57	1863	±	50	102	
17.1	e,osc,p	393	230	0.58	0.00257	±	0.00067	0.0424	5.128	±	0.376	0.0789	±	0.0121	1149	±	78	1170	±	338	98	
18.1	m,p	760	146	0.19	0.00067	±	0.00026	0.0111	4.906	±	0.317	0.0911	±	0.0047	1196	±	71	1448	±	101	83	
19.1	m,osc,p	384	31	0.08	0.00004	±	0.00002	0.0007	3.942	±	0.101	0.0901	±	0.0009	1457	±	33	1427	±	18	102	
20.1	m,hp,p	371	445	1.20	0.00040	±	0.00009	0.0065	5.668	±	0.149	0.0752	±	0.0019	1047	±	25	1073	±	51	98	
21.1	m,hp,p	168	119	0.71	0.00170	±	0.00029	0.0280	3.487	±	0.136	0.1056	±	0.0051	1625	±	56	1724	±	90	94	
22.1	e,osc,p	231	126	0.54	0.00094	±	0.00031	0.0154	2.905	±	0.211	0.1053	±	0.0051	1907	±	121	1720	±	91	111	
23.1	m,osc,p	118	143	1.21	0.00033	±	0.00016	0.0054	3.400	±	0.153	0.1085	±	0.0035	1662	±	66	1774	±	60	94	
24.1	h,p	833	421	0.51	0.00076	±	0.00023	0.0126	4.590	±	0.270	0.0830	±	0.0041	1271	±	68	1270	±	100	100	
																						
Analysis code: x.y = grain.site number																			
Habit and site: p= prism (aspect ratio >2), eq= equant, abr= rounded by transport, 										
e= end/edge, m= middle, r = overgrowth, c= core, fr= fragment, anh= anhedral,															
CL petrography: osc= fine-scale oscillatory zoning, sz= sector zoning, h= homogeneous, hb= homogeneous-bright,  hd= homogeneous-dark, rex= recrystallised				
All analytical errors are 1 sigma.																				
207Pb/206Pb and 206Pb/238U ages are after correction for common Pb using measured 206Pb/204Pb and Cumming & Richards (1975) model Pb composition for the likely age of the rock.	
f206 is the proportion of 206Pb that is non-radiogenic (common) in origin, based on measured 204Pb/206Pb and Cumming & Richards (1975) Pb evolution.				
In cumulative frequency diagrams analyses with f206>0.025 and with concordance (*) <90 or >110 are rejected. 											
Cumulative frequency diagrams are compiled using 207Pb/206Pb ages when these are >1000 Ma, and 206Pb/238U ages when the 207Pb/206Pb ages are <1000 Ma.